	Meganies
	 

	Is die spuitpomp goed gehak aan trekker?
	 

	Is daar enigiets fout met die spuitpomp raam?
	 

	Is die wiele en bande in 'n werkende toestand?
	 

	Is die PTO se kous vas en onbeskadig
	 

	Is die PTO gekoppel en vas?
	 

	Is die PTO gesmeer?
	 

	Hidroulies (die pomp en pype)
	 

	Is daar enige lek plekke onder druk?
	 

	Is daar enige barste of krake in een van die lyne?
	 

	Is alle krane en filters op die pype skoon?
	 

	Is die pomp gesmeer/geolie?
	 

	Spuit tenk
	 

	Is die tenk goed vas aan die spuit raam?
	 

	Enige lek plekke?
	 

	Is die deksel in goeie toestand en maak dit goed toe?
	 

	Is die tenk volume meter skoon en leesbaar?
	 

	Werk die meng stelsel?
	 

	Spuitkoppe
	 

	Sluit en draai die eenhede sonder lekkasie?
	 

	Anti drip" koppe in werkende toestand?
	 

	Is die spuitkoppe reg georiënteer?
	 

	Is die spuit kop uitleg reg van bo na onder?
	 

	Is enige spuitkoppe geblok?
	 

	Is elke spuit kop se spuit patroon reg?
	 

	Krane en meters
	 

	Werk die hoof kraan?
	 

	Werk die lyn krane?
	 

	Is die drukmeter leesbaar?
	 

	Tel die drukmeter druk op?
	 

	Is die drukmeter naald stabiel?
	 

	Filters
	 

	Alle filters gespoel?
	 

	Is die filters skoon?
	 

	Moet een van die filters vervang word?
	 

	Elektries
	 

	Is die bedrading onbeskadig?
	 

	Skop die elektriese krane oop?
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Operator Checklist for Canopy Sprayer
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Serial No.

Key: 7] Checked/Completed [XINeeds Attention /Adjusted [ Not Applicable

Regularly Check

Mechanical

(s the attachment to tractor secure?

(T Ave the chassis and structure free of
cracks and rust?

[ Are the wheels and tyres in good
condition?

[ Are guards, including PTO shaft
‘guard, secure and undamaged?

Hydraulic System
[is tfree from leaks under
pressure?

] Are the hoses and connections
wom or cracked?

Electrical System
[J1s the wiring undamaged and are
all connections properly insulated?

sprayer Tank

] A the tankichassis fasteners
secure?

[ Free from leaks?

[ Does the lid fit securely and is t free.
fromleaks?

(15 the contents gauge clearly legbie?

Spray Lines

[ Ave they free from leaks under
pressure?

[JNo hoses and connectors wom
or cracked?

[ Are all valves and fters in good
condition?

Nozzles

[C]Ave allitings in good condition?

5] Ave all nozzles correctly oriented?

(£ Ae all check valves working properly?

[CJ1s the sprayidistribution patter visually
correct?

Controls and Valves

[ Are the master onloff switches working
correctly?

[JAre left and right manifold switches
‘functioning?

[ Can you read the pressure gauge easily?

(] Are alllabels appropriate and legible?

[J1s the pressure adjustment stable?

[JPressure gauge reading zero?

Chemical Induction System (f fitted)

[ Are the system and controls working
properly?

[Jis tfree from leaks under pressure?

[0 Are all abels appropriate and readable?

D Are the rinse system and container wash
system working properly?

Tank Rinse System (if ftted)
(315 the system functioning properly?

Periodically Check
(] Calibration-Jug test all nozzle outputs.

Date completed
] Formally complete and file checkiist.

Comments/Notes/Specific ltems Requiring Attention:

coppight 2010 Andrew Landers, Efctive Vineand Speping.




